Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 118 - LIT-18626-11-77
P. 118

    SportsBoat_F3M12.book  Page 112  Monday, June 12, 2017  11:53 AM

                            Maintenance

                                                                           Initial  Thereafter every
                                                                                   50    100    200
                                    Item                Operation                 hours   hours   hours
                                                                            10
                                                                           hours  or 12   or 12   or 24
                                                                                 months  months  months
                                                                                   *1     *1     *1
                                               Check connections and exterior,
                             Steering cable                                               √
                                               and lubricate
                             Articulating keel  Check operation                           √
                                               Check exterior and operation, check
                             Remote control lever  shift operation, and check for loose-  √  √
                                               ness
                                               Check connections and exterior,
                             Throttle cable                                               √
                                               and lubricate
                                               Check connections and exterior,
                             Shift cable                                                  √
                                               and lubricate (shift gate end)
                             Exhaust hose, water   Check for exhaust leakage, and         √
                             lock, and resonator  check clamps at connections
                             Drain passages    Remove clogs                               √
                             Drain plugs       Check O-rings                 √            √
                             Hull and deck     Check for damage              √            √
                                               Check installation and operation,
                             Windshield and seats                            √            √
                                               and check for damage
                             T-top (190 FSH Sport)
                             and bimini top    Check installation, and check for   √      √
                             (190 FSH Sport/   damage
                             190 FSH Deluxe)
                             Hatches, hinges, and   Check installation       √            √
                             packing seals
                             Ladder            Check installation            √            √
                             Access port cap   Check exterior and installation            √
                             Spark plugs       Check                         √            √
                             High-pressure fuel   Check connections and exterior,         √
                             hose              and check for leakage
                             Engine oil        Replace                       √     √      √
                             Engine oil filter  Replace                                   √
                             Air filter element  Check for damage and dirt                √
                             Intake hose and   Check for damage, and check con-           √
                             breather hose     nections
                             Throttle body     Lubricate throttle valve                   √
                             Anode (engine)    Check for corrosion                              √ *2
                             Valve clearance   Check and adjust                                 √ *2
                             Rubber coupling   Check for looseness and noise                     √
                             Engine mount      Check for damage and peeling                      √
                             Cooling water hose   Check for damage, and check con-
                             and cooling water pi-  nections                                     √
                             lot outlet hose
                             Water inlet strainer  Check for damage          √            √
                             Intake grate      Check for damage              √            √

                            112

| 113 114 115 116 117 118 119 120 121 122 123 |