Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 88 - LIT-18626-11-77
P. 88

    UF3P11E0.book  Page 83  Wednesday, June 14, 2017  11:35 AM

                            Care and storage

                            EJU37146                              (3) Connect the garden hose  adapter to a
                                   Post-operation care
                                                                     garden hose.
                            EWJ00331
                                 WARNING
                            Always place the watercraft upright in a      1               2
                            horizontal position when storing it, other-
                            wise fuel could leak out into the engine or
                            engine compartment, which could create
                            a fire hazard.
                            After using the watercraft, always take it out
                            of the water, clean it, and store it. Leaving the
                            watercraft in the water for extended periods
                                                                   1 Garden hose adapter
                            will accelerate the rate of normal deteriora-
                                                                   2 Garden hose
                            tion of the jet pump and hull. Marine organ-
                            isms  and corrosion  are some of the  (4) Loosen the flushing hose connector cap
                            conditions that can shorten the life of many  and  remove  it. Insert the garden  hose
                            watercraft components.                   adapter into the flushing hose connector
                            EJU37566                                 by pushing and twisting it until it is se-
                            Flushing the cooling water passages      curely connected.
                            ECJ01880
                             NOTICE
                             Do not run the engine over 4000 r/min on
                              land. Also, do not run  the engine for
                                                                                2
                              more than 15 seconds without supplying
                              water, otherwise the engine could over-
                              heat.
                             Flush the cooling water passages to
                                                                                3
                              prevent them from  clogging with salt,
                              sand, or dirt.
                                                                                                1
                            (1) Place the watercraft in a horizontal posi-
                                tion.
                            (2) Remove the seats and removable water-
                                tight storage compartment. (See page 47
                                for seat removal and installation proce-
                                dures and page 52 for information on the
                                removable watertight storage compart-
                                ment.)

                                                                   1 Flushing hose connector cap
                                                                   2 Garden hose adapter
                                                                   3 Flushing hose connector

                            83

| 83 84 85 86 87 88 89 90 91 92 93 |