Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 89 - LIT-18626-11-77
P. 89

    UF3P11E0.book  Page 84  Wednesday, June 14, 2017  11:35 AM

                                                                           Care and storage

                            (5) Connect the garden hose to a water tap.  EJU33747
                                                                  Cleaning the watercraft
                            (6) Make sure that the area around the wa-
                                                                  (1) Remove the seats. (See page 47 for seat
                                tercraft is clear, and then start  the en-
                                                                     removal and installation procedures.)
                                gine. Immediately after the engine starts,
                                                                  (2) Rinse  the engine and engine compart-
                                fully turn the water supply on so that wa-
                                                                     ment with a small amount of  water.
                                ter flows out continually from  the  jet
                                                                     NOTICE: Do not use high-pressure
                                thrust nozzle.
                                                                     water when rinsing the engine or en-
                                                                     gine  compartment as severe engine
                                                                     damage could result. [ECJ00572]
                                                                  (3) Drain  the water  from the engine com-
                                                                     partment. (See page 58 for information
                                                                     on draining the bilge water.)
                                                                  (4) Wipe  the engine  and engine compart-
                                                                     ment with a dry cloth.
                                                                  (5) Wash down the hull, deck, and jet pump
                                                                     with fresh water.
                                                                  (6) Wipe the hull, deck, and jet pump with a
                            (7) Run the engine at idling speed for about
                                                                     dry cloth.
                                3 minutes watching the engine condition.
                                                                  (7) Wipe  all vinyl and rubber components,
                                If the  engine stops  while flushing,  turn
                                                                     such as the seats and engine compart-
                                the water supply off immediately  and
                                                                     ment seals, with a vinyl protectant such
                                perform the procedure again from step 6.
                                                                     as Yamaclean Vinyl Dressing™.
                                NOTICE: Do not supply water to the
                                                                  (8) To minimize corrosion, spray metallic
                                cooling water passages when the en-
                                                                     parts of the hull, deck, and engine with a
                                gine is not running. The water could
                                                                     rust inhibitor such as Yamalube Silicone
                                flow back through the muffler into the
                                                                     Protectant & Lubricant.
                                engine, causing severe engine  dam-
                                                                  (9) Allow the engine compartment to air dry
                                age. [ECJ00123]
                                                                     completely before installing the seats.
                            (8) Turn the water supply off.
                                                                  (10) Securely install the seats in their original
                            (9) Discharge the remaining water out of the
                                                                     positions.
                                cooling  water passages by  alternately  EJU41632
                                squeezing and releasing the throttle lever  Battery care
                                quickly for 10 to 15 seconds.     If the watercraft will not be used for more than
                            (10) Stop the engine.                 a month, remove the battery from the water-
                            (11) Remove the garden hose adapter, and  craft, check it, and then store it in a cool, dry
                                then securely install the flushing hose  place.
                                connector cap  by tightening  it until it  EWJ00792
                                                                      WARNING
                                stops.
                            (12) Securely install the removable watertight  Battery electrolyte is poisonous and dan-
                                storage compartment and seats in their  gerous, causing severe burns, etc. Elec-
                                original positions.
                                                                                                   84

| 84 85 86 87 88 89 90 91 92 93 94 |