Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 33 - LIT-18626-12-09
P. 33

    UF4D14E0.book  Page 28  Tuesday, March 27, 2018  1:02 PM

                                                                     Equipment operation

                            To install the hood:                  towing it in an emergency. (See page 72 for
                            (1) Position the hood on the deck so that the  information on towing the watercraft.)
                                two projections at the front of the hood fit
                                under the two stays on the deck.

                                                                     1
                                                                   1 Bow rope hole
                                                                  EJU36012
                                                                  Stern rope hole
                            (2) Push down on the hood latch, and then
                                                                  The stern rope hole is used to attach a rope
                                turn the knob to the “LOCK” position to
                                                                  to the watercraft when mooring it.
                                securely lock the hood in place.

                                                    LOCK  OPEN

                                                                   1 Stern rope hole
                            (3) While  holding the  steering pole, move  EJU31676
                                the lock pin to the stowed position, and  Storage pouch
                                then lower the steering pole.     The storage pouch is located on the bottom
                            EJU36003                              of the hood.
                            Bow rope hole                         Use the  storage pouch to  store the own-
                            The bow rope hole is used to attach a rope to  er’s/operator’s manual, tool  kit, and other
                            the watercraft when transporting, mooring, or  small  items. The storage pouch  is  not de-
                                                                  signed to be waterproof. If you carry objects
                                                                  that must be kept dry, put them in a water-
                                                                  proof bag.
                                                                  To remove the storage pouch:
                                                                  (1) Remove the hood. (See page 27 for hood
                                                                     removal and installation procedures.)

                                                                                                   28

| 28 29 30 31 32 33 34 35 36 37 38 |