Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 46 - LIT-18626-12-09
P. 46

    UF4D14E0.book  Page 41  Tuesday, March 27, 2018  1:02 PM

                            Pre-operation checks

                            Make sure that there is the proper amount of  EJU41021
                                                                  Switch checks
                            throttle lever free play when the throttle lever  ECJ01361
                            is in the fully closed (idle) position.  NOTICE
                                                                  Do not run  the engine for  more than 15
                                                                  seconds on land without supplying water,
                                                                  otherwise the engine could overheat.

                                                                  Check the start switch, the engine stop
                                                                  switch,  and the engine  shut-off switch  for
                                                                  proper operation. (See pages 23 to 23 for in-
                                                                  formation on operating each switch.)

                                                                              1     2     3
                              1 Throttle lever free play
                              Throttle lever free play:
                                7.0–10.0 mm (0.28–0.39 in)

                            EJU32664                                      4
                            Engine shut-off cord (lanyard) check
                            Make sure that the engine shut-off cord (lan-    5
                            yard) is not damaged. If the cord is damaged,
                            replace it.  WARNING! Never try to repair  1 Engine shut-off switch
                            the engine shut-off cord (lanyard) or tie it  2 Clip
                            together. The engine  shut-off cord (lan-  3 Start switch
                            yard) may not pull free when the operator  4 Engine stop switch
                            falls off, allowing the watercraft to conti-  5 Engine shut-off cord (lanyard)
                            nue to run and cause an accident. [EWJ01221]  To check the operation of the switches:
                                                                  (1) Push the start switch to make sure that
                                                                     the engine starts.
                                                                  (2) As  soon as the  engine starts running,
                                                                     push the engine stop switch to  make
                                                                     sure that the engine stops immediately.
                                                                  (3) Restart the engine, and then pull the en-
                                                                     gine  shut-off cord (lanyard) to  remove
                                                                     the clip from the engine shut-off switch
                                                                     to make sure that the engine stops im-
                                                                     mediately.
                                                                  EJU41211
                                                                  Storage pouch checks
                                                                  Make sure that the storage pouch is not dam-
                                                                  aged and that water has not collected in the
                                                                  pouch. Also, make  sure that the  storage

                            41

| 41 42 43 44 45 46 47 48 49 50 51 |