Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 65 - LIT-18626-12-09
P. 65

    UF4D14E0.book  Page 60  Tuesday, March 27, 2018  1:02 PM

                                                                                 Maintenance

                            EJU41751                              carry it with you whenever you use the water-
                                       Maintenance
                                                                  craft.
                            Periodic  checks and  lubrication will keep
                            your watercraft in the safest and most effi-
                            cient condition  possible. Therefore, make
                            sure to carry out the periodic maintenance.
                            Safety is an obligation of the watercraft own-
                            er. The most important points of watercraft
                            inspection and lubrication are explained on
                            the following pages.
                            See a Yamaha dealer for genuine Yamaha re-
                            placement parts and  optional accessories
                            designed for your watercraft.          1 Tool bag
                            EWJ00312                               2 Screwdriver
                                 WARNING                           3 10/12 mm box wrench
                            Be sure to turn off the engine when you  4 Spark plug (one included for each cylinder)
                            perform maintenance  unless otherwise  5 14/21 mm box wrench
                            specified. If you are not familiar with ma-  6 Pliers
                                                                   7 10/12 mm open-end wrench
                            chine servicing, this work should be done
                            by a Yamaha dealer or other qualified me-  EJU34338
                                                                  Adjusting the steering friction
                            chanic.
                                                                  The amount of friction in the steering can be
                            A service  manual is  available for  purchase  adjusted to suit operator preference.
                            through a  Yamaha dealer  for owners  who  To adjust the steering friction:
                            have the mechanical skills, tools, and other  (1) Lift the steering pole and support it with
                            equipment necessary to perform  mainte-  the lock pin.
                            nance not covered by this owner’s/operator’s
                            manual.
                            EJU33803
                            Tool kit
                            A tool kit is included with this watercraft. Pla-
                            ce the tool kit in a waterproof bag and always

                                                                   1 Steering pole
                                                                   2 Lock pin

                                                                                                   60

| 60 61 62 63 64 65 66 67 68 69 70 |