Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 29 - LIT-18626-12-09
P. 29

    UF4D14E0.book  Page 24  Tuesday, March 27, 2018  1:02 PM

                                                             Control function operation

                            will not start. Also, the starter motor could  zle is changed, and the direction of the water-
                            be damaged. [ECJ01041]                craft is changed accordingly.

                                                   1

                                               START

                              1 Start switch                       1 Handlebar
                                                                   2 Jet thrust nozzle
                            The engine will not start when the clip is re-
                            moved from the engine shut-off switch.  Since the strength of the jet thrust determines
                            EJU31212                              the speed and degree of a turn, throttle must
                            Throttle lever                        always be applied when attempting a turn,
                            The throttle lever increases the engine speed
                                                                  except at trolling speed.
                            when the lever is squeezed.
                                                                  The angle of the jet thrust nozzle can be ad-
                                                                  justed to suit operator preference. (See page
                                                                  61 for information on adjusting the jet thrust
                                                                  nozzle angle.)
                                                                  EJU31273
                                                                  Steering pole
                                                                  The steering pole can be moved up or down
                                                                  to change the height of the handlebars.

                              1 Throttle lever
                            The throttle lever returns automatically to its
                            fully closed (idle) position when released.
                            EJU35933
                            Steering system
                            By turning the handlebars in the direction you
                            wish to travel, the angle of the jet thrust noz-

                                                                                                   24

| 24 25 26 27 28 29 30 31 32 33 34 |