Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 52 - LIT-18626-12-09
P. 52

    UF4D14E0.book  Page 47  Tuesday, March 27, 2018  1:02 PM

                            Operation

                                lision or  cause the operator to be  dental starting or unauthorized operation by
                                thrown overboard. [EWJ00592]      children or others.

                                               START                                STOP

                            (6) After the engine has warmed up, push  EJU41172
                                                                  Operating the watercraft
                                the choke knob in to its original position.
                                                                  When the  engine is running, the  watercraft
                            TIP:                                  will move forward at trolling speed even if the
                            If the choke knob is left pulled out, the engine  throttle lever is in the fully closed (idle) posi-
                            will stall.                           tion.
                            EJU32863
                            Stopping the engine
                            Release the throttle lever, and then push the
                            engine stop switch (red button) to stop the
                            engine.  WARNING!  You need throttle  to
                            steer. Shutting  the engine off can  cause
                            you to hit an obstacle you are attempting
                            to avoid. A collision could result in severe
                            injury or death. [EWJ00602]

                                                                  EJU33244
                                                                  Turning the watercraft
                                                                  EWJ00762
                                                                      WARNING
                                                                   Do not release the throttle lever when
                                                                   trying to steer away from objects—you
                                                                   need throttle to steer. A collision could
                                                                   result in severe injury or death.
                                                                   When operating at higher speeds, make
                            EJU32873                               gradual turns or slow down before turn-
                            Leaving the watercraft
                                                                   ing. Sharp high-speed turns may cause
                            If leaving the watercraft, remove the clip from
                                                                   the watercraft to slide sideways or spin,
                            the  engine shut-off switch  to prevent  acci-
                                                                   throwing the operator overboard, which
                                                                   could cause an injury.

                            47

| 47 48 49 50 51 52 53 54 55 56 57 |