Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 47 - LIT-18626-12-09
P. 47

    UF4D14E0.book  Page 42  Tuesday, March 27, 2018  1:02 PM

                                                                    Pre-operation checks

                            pouch is securely installed. (See page 28 for  EJU32353
                                                                  Hull and deck check
                            information on the storage pouch.)
                                                                  Check the hull and deck for damage or other
                            EJU41072
                            Fire extinguisher container checks    problem.
                            Make sure that the fire extinguisher container  EJU32657
                                                                  Jet intake checks
                            is not damaged and is securely held in place.
                                                                  Make sure that the jet intake is not damaged
                            (See page 29 for information on the fire extin-
                                                                  or clogged with weeds or debris. If the jet in-
                            guisher container.)
                                                                  take is clogged, clean it. (See page 70 for in-
                            EJU32494
                            Fire extinguisher check               formation on the jet intake.)
                            Check that there is a full fire extinguisher on  EJU40703
                                                                  Hood check
                            board.
                                                                  Make sure that the hood is securely closed.
                                                                  (See page 27 for information on the hood.)

                            To check  the  fire extinguisher, see the  in-
                            structions supplied  by the fire extinguisher
                                                                  EJU40146
                            manufacturer. Always keep the fire extin-  Post-launch checks
                            guisher in the fire extinguisher container.  Perform the post-launch checks in the pre-
                            Always carry a fire extinguisher on board. A  operation checklist while the watercraft is in
                            fire extinguisher is not standard  equipment  the water and the engine is running.
                            with this watercraft. If you do not have one,  To perform the post-launch checks:
                            contact a Yamaha dealer or a fire extinguish-  (1) Launch the watercraft. (See page 45 for
                            er dealer to obtain one meeting the proper  information on launching the watercraft.)
                            specifications.                       (2) Perform the checks and make sure that
                                                                     there are no malfunctioning items or oth-
                              Fire extinguisher:                     er problems.
                                Classification:
                                                                  EJU40553
                                  B-1                             Cooling water pilot outlet check
                                Capacity:                         Make sure that water is discharged from the
                                  2 lb or more
                                                                  cooling water pilot outlet while the engine is
                            EJU40122
                            Safety equipment check
                            Check that safety equipment meeting the ap-
                            plicable regulations is on board.

                                                                                                   42

| 42 43 44 45 46 47 48 49 50 51 52 |