Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 35 - LIT-18626-12-09
P. 35

    UF4D14E0.book  Page 30  Tuesday, March 27, 2018  1:02 PM

                                                                     Equipment operation

                            (4) Loosen  the fire extinguisher container
                                cap and remove it.

                              1 Fire extinguisher container cap
                            To close the fire extinguisher container:
                            (1) Insert the fire extinguisher into the con-
                                tainer, and then securely install the fire
                                extinguisher container cap by tightening
                                it until it stops.
                            (2) Lower the container on the hood to its
                                storage position  and secure  it with the
                                band.
                            (3) While  holding the  steering pole, move
                                the lock pin to the stowed position, and
                                then lower the steering pole.

                                                                                                   30

| 30 31 32 33 34 35 36 37 38 39 40 |