Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 30 - LIT-18626-12-09
P. 30

    UF4D14E0.book  Page 25  Tuesday, March 27, 2018  1:02 PM

                            Control function operation

                            EJU31124                              fuel while operating the watercraft. When this
                            Fuel cock knob
                                                                  occurs, refuel as soon as possible and be
                            The fuel supply method can be switched by
                                                                  sure to turn the fuel cock knob back to “ON”.
                            operating the fuel cock knob.
                                                                  EJU31203
                            Select the fuel cock knob position from the  Choke knob “  ”
                            following three positions according to the cir-  The choke knob can be operated to supply a
                            cumstances of use.                    richer air-fuel mixture that is required to start
                                                                  a cold engine.
                                                                  To use the choke:
                                                                  Pull the choke knob out.
                                                                  Push the  choke knob  in  to stop using the
                                                                  choke after the engine starts.

                              1 Fuel cock knob

                                                                   1 Choke knob
                                                                  EJU31224
                                                                  Cooling water pilot outlet
                                                                  When the engine  is running, some of the
                                                                  cooling water that is circulated in the engine
                                                                  is discharged from  the cooling  water pilot
                                                                  outlet.
                            OFF:
                            With the fuel cock knob in this position, fuel
                            does not flow to the carburetors. Always turn
                            the fuel cock knob to this position when the
                            engine is not running.
                            ON:
                            With the fuel cock knob in this position, fuel
                            flows to the carburetors. Turn the fuel cock
                            knob to this position when starting the engine
                            and operating the watercraft.
                            RES:
                                                                   1 Cooling water pilot outlet
                            With the fuel cock knob in this position, the
                                                                  There is a cooling water pilot outlet on the
                            fuel reserve is made available. Turn the fuel
                                                                  port (left) side of the watercraft. To check for
                            cock knob to this position if you run out of
                            25

| 25 26 27 28 29 30 31 32 33 34 35 |