Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 32 - LIT-18626-12-09
P. 32

    UF4D14E0.book  Page 27  Tuesday, March 27, 2018  1:02 PM

                            Equipment operation

                            EJU40334                              (2) Turn the latch knob to the “OPEN” posi-
                                        Equipment
                                                                     tion, and then pull up on the hood latch
                            EJU31057
                            Hood                                     to unlatch the hood.
                            The hood is removable.
                            Remove the hood to access the engine com-
                            partment.                               1
                            To remove the hood:
                            (1) Lift the steering pole and support it with
                                the lock pin.
                                                                        LOCK  OPEN
                                                                    2

                                                                   1 Hood latch
                                                                   2 Hood latch knob
                                                                  (3) Grasp the hood using the handgrips pro-
                                                                     vided at the front and rear of the hood.
                                                                     Lift the hood up and to the rear to re-
                                                                     move it.
                              1 Steering pole

                                                                   1 Handgrip
                              1 Lock pin

                            27

| 27 28 29 30 31 32 33 34 35 36 37 |