Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 76 - LIT-18626-12-09
P. 76

    UF4D14E0.book  Page 71  Tuesday, March 27, 2018  1:02 PM

                            Trouble recovery

                            (2) Remove any weeds  or  debris from  (3) Connect the other end of the negative (–)
                                around the jet intake, drive shaft, impel-  jumper cable to an unpainted bolt on the
                                ler, jet pump housing, and jet thrust noz-  cylinder head.
                                zle.
                                If debris is difficult to remove, consult a
                                Yamaha dealer.
                            EJU34642
                            Jumping the battery
                            If the watercraft battery has run down, the en-
                            gine can be started using a 12-volt booster
                            battery and jumper cables.
                            EJU34654
                            Connecting the jumper cables
                            EWJ01251
                                 WARNING                           1 Positive (+) jumper cable
                            To avoid  battery  explosion and serious  2 Booster battery
                            damage to the electrical system:       3 Negative (–) jumper cable
                             Do not reverse the polarity of the jumper  (4) Start the engine, and then disconnect the
                              cables when connecting to the batter-  jumper cables by reversing  the  steps
                              ies.                                   above. (See page 23 for information on
                             Do not connect the negative (–) jumper  starting the engine.)
                              cable to the negative (–) terminal of the  EJU34676
                                                                  Replacing the fuse
                              watercraft battery.
                                                                  If the fuse is blown, replace it with the proper
                             Do not touch the positive (+) jumper ca-
                                                                  fuse.
                              ble to the negative (–) jumper cable.
                                                                    1                2
                            (1) Connect the positive (+) jumper cable to
                                the positive (+) battery terminals of both
                                batteries.
                            (2) Connect one  end of the negative  (–)
                                jumper cable to the negative (–) battery
                                terminal of the booster battery.

                                                                   1 Good fuse
                                                                   2 Blown fuse
                                                                  To replace the fuse:
                                                                  (1) Remove the hood. (See page 27 for hood
                                                                     removal and installation procedures.)
                                                                  (2) Loosen the cap and remove it.
                                                                  (3) Pull out the red lead to pull out the fuse
                                                                     holder from the electrical box.

                            71

| 71 72 73 74 75 76 77 78 79 80 81 |