Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 64 - LIT-18626-12-09
P. 64

    UF4D14E0.book  Page 59  Tuesday, March 27, 2018  1:02 PM

                            Care and storage

                             Steering cable ball joint (jet thrust nozzle  (4) Run the engine at a fast idle.
                              end)  and  steering cable inner wire (jet  (5) Quickly spray as much rust inhibitor as
                              thrust nozzle end)                     possible through the hole in the silencer
                                                                     cover. Use Yamalube  Stor-Rite  Engine
                                                                     Fogging  Oil or an equivalent. Keep
                                                                     spraying until the engine stalls (or a maxi-
                                                                     mum of 15 seconds). WARNING! Do not
                                                                     pour or spray  gasoline,  or any sub-
                                                                     stance other  than a rust  inhibitor
                                                                     through the hole in the silencer cover.
                                                                     Do not spray flammable rust inhibitor
                                                                     products on engine surfaces while the
                                                                     engine is hot. Otherwise, a fire or ex-
                            EJU40935                                 plosion could occur. [EWJ00302]
                            Rustproofing
                                                                  (6) Securely install the silencer cap by tight-
                            ECJ01361
                             NOTICE                                  ening it until it stops. NOTICE: Be sure
                                                                     to install the silencer cap securely af-
                            Do not run the engine for more than 15
                                                                     ter fogging the engine, otherwise wa-
                            seconds on land without supplying water,
                                                                     ter could enter the engine and cause
                            otherwise the engine could overheat.
                                                                     damage. [ECJ00153]
                            Spray metallic parts of the hull and engine  (7) Securely install the hood in its original
                            with a rust inhibitor such as Yamalube Sili-  position.
                            cone Protectant & Lubricant.
                            To rustproof the internal engine components:
                            (1) Remove the hood. (See page 27 for hood
                                removal and installation procedures.)
                            (2) Loosen the silencer cap and remove it.

                              1 Silencer cap
                            (3) Make sure that the area around the wa-
                                tercraft is clear, and then start the engine
                                in a well-ventilated area.

                            59

| 59 60 61 62 63 64 65 66 67 68 69 |