Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 66 - LIT-18626-12-09
P. 66

    UF4D14E0.book  Page 61  Tuesday, March 27, 2018  1:02 PM

                            Maintenance

                            (2) Remove the  four screws, and  then re-  (8) While holding the steering pole, move
                                move the handlebar cover.            the lock pin to the stowed position, and
                                                                     then lower the steering pole.
                                                                  EJU3128A
                                                                  Adjusting the jet thrust nozzle angle
                                                                  The angle of the jet thrust nozzle can be ad-
                                                                  justed to two settings to suit operator prefer-
                                                                  ence.
                                1                                 To adjust the jet thrust nozzle angle:
                                                                  (1) Remove the two bolts, and then remove
                                                                     the steering pole cover.

                              1 Handlebar cover
                            (3) Turn the handlebars so that the left han-
                                dlebar grip is facing down.
                            (4) Loosen the locknut.
                            (5) Tighten or loosen the adjusting nut until
                                the desired  amount  of friction is  ob-
                                tained.

                                                                   1 Steering pole cover
                                                                  (2) Pull back the outer sleeve of the steering
                                                                     cable joint, and then disconnect the joint
                                                                     from the steering cable pivot bolt.

                              1 Adjusting nut
                              2 Locknut
                            (6) While holding  the adjusting nut with  a
                                wrench, tighten the locknut to the speci-
                                fied torque.
                              Tightening torque:                   1 Steering cable joint
                                Locknut:
                                  28 N·m (2.8 kgf·m, 21 lb·ft)
                            (7) Securely install the handlebar cover and
                                four screws in their original positions.

                            61

| 61 62 63 64 65 66 67 68 69 70 71 |