Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 39 - LIT-18626-12-09
P. 39

    UF4D14E0.book  Page 34  Tuesday, March 27, 2018  1:02 PM

                                             Operation and handling requirements

                            EJU33424                              where they touch the body of the water-
                                       Transporting
                                                                  craft to avoid scratches or damage. [ECJ00633]
                            EWJ00751
                                 WARNING
                            Always turn the fuel cock knob to “OFF”
                            when transporting the watercraft, other-
                            wise fuel could leak out into the engine or
                            engine compartment, which would create
                            a fire hazard.

                                                                   1 Rubber shock cord
                                                                   2 Tie down

                            When transporting the watercraft on a trailer,
                            secure the bow rope hole  and stern of the
                            watercraft  to the trailer  with  ropes or tie
                            downs. Use a rubber shock cord to secure
                            the steering pole to the watercraft. NOTICE:
                            Do not secure the steering pole with ropes
                            or tie downs and do not secure it to the
                            trailer. Also, do not transport the water-
                            craft with the steering pole up. Otherwise,
                            the steering pole could be damaged. Wrap
                            the ropes or tie downs with towels or rags

                                                                                                   34

| 34 35 36 37 38 39 40 41 42 43 44 |