Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 75 - LIT-18626-12-09
P. 75

    UF4D14E0.book  Page 70  Tuesday, March 27, 2018  1:02 PM

                                                                           Trouble recovery

                            EJU34625                              ways stop the engine before beaching  the
                                 Emergency procedures
                                                                  watercraft.
                            EJU34635
                            Cleaning the jet intake and impeller
                            EWJ00783
                                 WARNING
                            Before attempting to remove weeds or de-
                            bris  from the jet intake or  impeller area,
                            shut the engine off and  remove  the  clip              STOP
                            from the engine shut-off switch. Severe in-
                            jury or death could result from coming in
                            contact with the rotating parts of the jet
                            pump.
                            If weeds or debris gets caught in the jet intake
                            or impeller, cavitation can occur, causing jet
                            thrust to decrease even though engine speed
                            rises. If this condition is allowed to continue,
                            the  engine will overheat and  may  seize.
                            NOTICE: If weeds or debris gets caught in
                            the jet intake, do not operate the water-
                            craft above trolling speed until they have
                            been removed. [ECJ00654]
                            If there is any sign that the jet intake or impel-  (1) Place a suitable clean cloth or carpeting
                            ler is clogged with weeds or debris, return to  underneath the watercraft  to protect  it
                            shore and check the intake and impeller. Al-  from abrasions and scratches. Turn the
                                                                     watercraft on its  side as shown.
                                                                     NOTICE: Always  turn the watercraft
                                                                     over onto its  port  (left) side. When
                                                                     turning the watercraft on its side, sup-
                                                                     port the bow so that the handlebars
                                                                     are not bent or damaged. [ECJ00662]

                                                                                                   70

| 70 71 72 73 74 75 76 77 78 79 80 |