Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 42 - LIT-18626-12-09
P. 42

    UF4D14E0.book  Page 37  Tuesday, March 27, 2018  1:02 PM

                            Pre-operation checks

                                      ITEM                         ROUTINE                   PAGE
                             POST-LAUNCH CHECKS
                                                    Check that water is discharged from the cooling
                             Cooling water pilot outlet                                       42
                                                    water pilot outlet while the engine is running.
                            TIP:
                            To ensure safety and reliability, pre-operation checks should be made each time the water-
                            craft is used.

                            37

| 37 38 39 40 41 42 43 44 45 46 47 |