Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 113 - LIT-18626-12-10
P. 113

    UF3V10E0.book  Page 108  Thursday, August 23, 2018  9:17 AM

                                                                           Trouble recovery

                            (1) Connect the positive (+) jumper cable to  EJU43482
                                                                  Replacing the fuses
                                the positive (+) battery terminals of both
                                                                  If a fuse is blown, replace it with the proper
                                batteries.
                                                                  fuse.
                            (2) Connect one  end of the negative  (–)
                                jumper cable to the negative (–) battery  1          2
                                terminal of the booster battery.
                            (3) Connect the other end of the negative (–)
                                jumper cable to an engine hanger.
                                                   2
                                1
                                                           3

                                            4
                                                                   1 Good fuse
                                                                   2 Blown fuse

                                                                    1                2
                              1 Negative (–) jumper cable
                              2 Booster battery
                              3 Positive (+) jumper cable
                              4 Engine hanger
                            (4) Start the engine, and then disconnect the
                                jumper cables by reversing  the  steps
                                above. (See page 32 for information on
                                starting the engine.)
                                                                   1 Good fuse
                                                                   2 Blown fuse
                                                                  To replace a fuse:
                                                                  (1) Remove the seats and removable water-
                                                                     tight storage compartment. (See page 55
                                                                     for seat removal and installation proce-
                                                                     dures and page 60 for information on the
                                                                     removable  watertight storage compart-
                                                                     ment.)
                                                                  (2) While  pushing the projection on  each
                                                                     lock, slide the locks outward.

                                                                                                 108

| 108 109 110 111 112 113 114 115 116 117 118 |