Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 82 - LIT-18626-12-10
P. 82

    UF3V10E0.book  Page 77  Thursday, August 23, 2018  9:17 AM

                            Pre-operation checks

                            and down properly and that the trim setting  EJU32534
                                                                  Fire extinguisher check
                            indicator and displayed setting level change
                                                                  Check that there is a full fire extinguisher on
                            according to the operation of the switches.
                                                                  board.
                            (See page 46 for information on turning on
                            the multifunction information center without
                            starting the engine and page 38 for informa-
                            tion on the electric trim system.)

                               0                                  To check the fire  extinguisher, see  the  in-
                                                                  structions supplied by the fire extinguisher
                                                                  manufacturer. Always keep the fire extin-
                                                                  guisher secured in the holder with its cover in
                            EJU40102
                            Storage compartment checks            place.
                            Make  sure that  the storage compartments  Always carry a fire extinguisher on board. A
                            are not damaged and that water has not col-  fire extinguisher is not  standard  equipment
                            lected in the compartments. (See page 58 for  with this watercraft. If you do not have one,
                            information on the storage compartments.)  contact a Yamaha dealer or a fire extinguish-
                            EJU41082                              er dealer to obtain one meeting the proper
                            Fire extinguisher holder, cover, and band
                                                                  specifications.
                            checks
                            Make sure that the fire extinguisher holder,  Fire extinguisher:
                            cover, and band are not damaged and that  Classification:
                            the cover is securely held in place using the  B-1
                            band. (See page 61 for information on the fire  Capacity:
                                                                        2 lb or more
                            extinguisher holder, cover, and band.)
                                                                  EJU40122
                                                                  Safety equipment check
                                                                  Check that safety equipment meeting the ap-
                                                                  plicable regulations is on board.
                                                                  EJU32353
                                                                  Hull and deck check
                                                                  Check the hull and deck for damage or other
                                                                  problem.

                            77

| 77 78 79 80 81 82 83 84 85 86 87 |