Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 43 - LIT-18626-12-10
P. 43

    UF3V10E0.book  Page 38  Thursday, August 23, 2018  9:17 AM

                                                                      Watercraft operation

                            TIP:                                  This function can be used only for  forward
                            If the RiDE lever is squeezed while the throttle  operation of the watercraft.
                            lever is squeezed, the  watercraft  will  slow  TIP:
                            down, and once stopped, move in reverse.   When the watercraft is moving in reverse or
                            To shift into neutral from forward:    is in neutral, the jet thrust nozzle will auto-
                            (1) Release the throttle lever.        matically change to the neutral trim setting.
                            (2) Lightly squeeze and release the RiDE le-  When the watercraft is shifted into forward,
                                ver. The “N” (neutral) shift indicator will  the  jet thrust nozzle will  automatically
                                be displayed.                      change to the selected trim setting.
                                                                   While the watercraft is in neutral,  the
                                                                   “TRIM/T.D.E.” switches control the forward
                                                                   and reverse operation of the T.D.E. (thrust
                                                                   direction enhancer). (See page 40 for infor-
                                                                   mation on the T.D.E.)
                                                                   The watercraft performance characteristics
                                                                   according to the trim angle change de-
                                                                   pending on the operating conditions.
                                                                  Confirming the trim setting
                                                                  The trim setting can be confirmed by the trim
                                                                  setting indicator and trim setting level on the
                                                                  multifunction information center.
                                                                    2  1
                                                     MPH

                               0                          100%
                                13.6V           x100       N                               MPH
                                                RPM
                                                           1        +2                          100%
                              1 “N” (Neutral position)
                                                                     13.6V           x100       F
                            TIP:                                   1 Trim setting indicator  RPM
                            If the RiDE lever is squeezed continuously,  2 Trim setting level
                            the reverse gate will move to the reverse po-
                                                                  To change the trim setting:
                            sition.
                                                                  (1) Shift into forward.
                            EJU45041
                            Electric trim system                  (2) Push the “TRIM/T.D.E.” up switch to in-
                            The  electric trim system is a  function for  crease the trim setting and raise the bow,
                            changing the vertical angle of the jet thrust  or push the “TRIM/T.D.E.” down switch
                            nozzle to change the trim angle and perfor-  to decrease the trim setting and lower
                            mance characteristics of the watercraft.

                                                                                                   38

| 38 39 40 41 42 43 44 45 46 47 48 |