Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 60 - LIT-18626-12-10
P. 60

    UF3V10E0.book  Page 55  Thursday, August 23, 2018  9:17 AM

                            Equipment operation

                            EJU40335                              To install the rear seat:
                                        Equipment
                                                                  (1) Insert the projections on the front of the
                            EJU45210
                            Seats                                    seat into the stays on the deck.
                            The front and rear seats are removable.
                            Remove the seats to access the engine com-
                            partment and removable watertight storage
                            compartment.
                            To remove the rear seat:
                            (1) Pull the rear seat latch up, and then lift up
                                the rear of the seat.

                                                          1
                                                                  (2) Push the rear of the seat down to secure-
                                                                     ly lock it in place.

                              1 Seat latch
                            (2) Pull the seat rearward and remove it.

                                                                  To remove the front seat:
                                                                  (1) Remove the rear seat.
                                                                  (2) Pull the front seat latch up, and then lift
                                                                     up the rear of the seat.

                                                                                         1

                                                                   1 Seat latch

                            55

| 55 56 57 58 59 60 61 62 63 64 65 |