Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 46 - LIT-18626-12-10
P. 46

    UF3V10E0.book  Page 41  Thursday, August 23, 2018  9:17 AM

                            Watercraft operation

                            This function can be used only when the wa-  TIP:
                            tercraft is in neutral.               While the T.D.E. is activated, the “N” (neutral)
                            TIP:                                  shift indicator will be displayed and “0” will be
                            While the watercraft is shifted into forward,  displayed on the speedometer.
                            the “TRIM/T.D.E.” switches control the elec-  To deactivate the T.D.E.:
                            tric trim system. (See page 38 for information  Perform one of the following operations. The
                            on the electric trim system.)         T.D.E. indicator disappears and the T.D.E. is
                            Activating and deactivating the T.D.E.  deactivated.
                            The activation of the T.D.E. can be confirmed   Squeeze the throttle lever.
                            by the T.D.E. indicator on the multifunction   Squeeze the RiDE lever.
                            information center.                    Push and hold  the  “NO-WAKE MODE”
                                                                   switch.
                                         2    T.D.E. FORWARD       While moving forward at a very low speed,
                                         3    T.D.E. REVERSE       push the “TRIM/T.D.E.” down switch.
                                                                   While moving in reverse at a very low
                                                     MPH           speed, push the “TRIM/T.D.E.” up switch.
                                      T.D.E. FORWARD              TIP:
                               0                          100%
                                                                  The T.D.E. is also deactivated when the en-
                                13.6V           x100       N      gine is stopped.
                                                RPM
                                                                  EJU45051
                                             1                    No-wake mode
                              1 T.D.E. indicator                  The no-wake mode is a function that main-
                              2 Forward operation at a very low speed  tains the engine speed at a fixed setting for
                              3 Reverse operation at a very low speed  operating the watercraft at low speeds. While
                            To activate the T.D.E.:               the watercraft is operating in no-wake mode,
                            (1) Shift into neutral.               the engine speed can be adjusted to one en-
                            (2) Push the “TRIM/T.D.E.” up switch to  gine speed each above and below the initial
                                move  forward at  a very  low speed or  engine speed.
                                push the “TRIM/T.D.E.” down switch to  This function can be used only when the wa-
                                move in reverse at a very low speed.  tercraft is in neutral, or when the watercraft is
                                                                  shifted into forward and the engine is operat-
                                                                  ing at idling speed.
                                                                  TIP:
                                                                  If the no-wake mode is activated when the
                                                                  watercraft is in neutral, the watercraft will au-
                                                                  tomatically shift into forward and the water-
                                                                  craft will start moving at a low speed.
                                          1
                                              2
                              1 “TRIM/T.D.E.” up switch
                              2 “TRIM/T.D.E.” down switch

                            41

| 41 42 43 44 45 46 47 48 49 50 51 |