Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 86 - LIT-18626-12-10
P. 86

    UF3V10E0.book  Page 81  Thursday, August 23, 2018  9:17 AM

                            Operation

                            jects, and other watercraft. Be  alert for  EJU32803
                                                                  Launching the watercraft
                            conditions that  limit  your visibility or block
                                                                  When launching the watercraft,  make  sure
                            your vision of others.
                                                                  that there are no obstacles around you.
                            You should grip  the handlebars  firmly  and
                                                                  If the watercraft is launched from a trailer,
                            keep both feet on the floor of the footwell. Do
                                                                  someone should make sure that waves do
                            not attempt to ride with passengers until your
                                                                  not push the watercraft into the trailer.
                            operating skills are fully developed.
                                                                  EJU36346
                            EJU40212                              Starting the engine on water
                            Riding position
                                                                  EWJ01531
                            Operator riding position                  WARNING
                            The operator should grip the handlebars firm-
                                                                  Do not apply throttle when anyone is at the
                            ly with both hands and sit astride the seat
                                                                  rear of the watercraft. Turn the engine off
                            with both feet on the floor of the footwell.
                                                                  or keep it at idle. Water and debris exiting
                                                                  the jet thrust nozzle can cause severe in-
                                                                  jury.
                                                                  To start the engine:
                                                                  (1) If the lock mode is selected for the
                                                                     Yamaha Security System setting, select
                                                                     the unlock mode. (See  page 31 for
                                                                     Yamaha Security System setting proce-
                                                                     dures.)
                                                                  (2) Move the  watercraft to an  area  that is
                            Passenger riding position                free from weeds and debris, and has a
                            The passenger(s) should hold on firmly, either  water depth of at least 60 cm (2 ft) from
                            to the person in front of them or to the hand-  the bottom of the watercraft. NOTICE:
                            grip provided, and sit astride the seat with  Never run the engine in water that is
                            their feet on the floor of the footwell. Never al-  less than 60 cm (2 ft) deep from the
                            low a passenger to ride in front of the opera-  bottom  of the watercraft, otherwise
                            tor. (See page 18 for information on the riding  pebbles or sand could be sucked into
                            position when pulling a wakeboarder or wa-  the jet intake, causing impeller dam-
                            ter-skier.)                              age and engine overheating. [ECJ00473]

                            81

| 81 82 83 84 85 86 87 88 89 90 91 |