Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 45 - LIT-18626-12-10
P. 45

    UF3V10E0.book  Page 40  Thursday, August 23, 2018  9:17 AM

                                                                      Watercraft operation

                            EJU40002                                 increase. The engine speed can be ad-
                              Watercraft operation modes
                                                                     justed to two levels: +1 and +2.
                            EJU45061
                            Reverse assist                                            1
                            The reverse assist is a function for temporar-
                            ily increasing the engine speed when moving
                            in  reverse,  such as to  enter the water
                            smoothly when launching the watercraft from
                            a trailer.
                            This function operates after the  engine is
                            started and only if the watercraft is not shifted
                            into forward.
                                                                   1 RiDE lever
                            TIP:
                            Once the watercraft is shifted into forward af-
                            ter the engine is started, the reverse assist
                            cannot be operated.                                              1
                            Activating and deactivating the reverse
                            assist                                                           2
                            The activation of  the reverse assist  can be
                            confirmed by the reverse assist indicator on
                            the multifunction information center.

                                                                   1 “SPEED CONTROL” up switch
                                                                   2 “SPEED CONTROL” down switch
                                                     MPH          To deactivate the reverse assist:
                                                                  Perform one of the following operations. The
                                     Reverse Assist  +2
                               0                          100%    beeper sounds two times and the reverse as-
                                                                  sist indicator disappears when  the reverse
                                13.6V           x100       R
                                                RPM               assist is deactivated.
                                            1        2             Relax your grip on the RiDE lever.
                              1 Reverse assist indicator           Push the “SPEED CONTROL” down switch
                              2 Reverse assist level               when the reverse assist level is set to +1.
                            To activate the reverse assist:        Squeeze the throttle lever.
                                                                  EJU45071
                            (1) Start the engine.
                                                                  T.D.E. (thrust directional enhancer)
                            (2) Squeeze the RiDE lever to the fully open  The T.D.E. is a function for slightly lifting or
                                position, and then push the “SPEED  lowering the reverse gate from the neutral po-
                                CONTROL” up switch. Once the beeper  sition to operate the watercraft at very low
                                sounds once and the reverse assist indi-  speeds when the engine is running at idling
                                cator is displayed, the engine speed will  speed.

                                                                                                   40

| 40 41 42 43 44 45 46 47 48 49 50 |