Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 37 - LIT-18626-12-10
P. 37

    UF3V10E0.book  Page 32  Thursday, August 23, 2018  9:17 AM

                                                             Control function operation

                            EJU31153                              vent accidental starting or unauthorized op-
                            Engine stop switch “ ”
                                                                  eration by children or others.
                            The engine stop switch (red button) stops the
                            engine when the switch is pushed.

                                           1
                                                                  EJU42323
                                                                  Start switch “  ”
                              1 Engine stop switch
                                                                  ECJ01311
                                                                  NOTICE
                            EJU31164
                            Engine shut-off switch “  ”           Do not run the engine over 4000 r/min on
                            The  engine shut-off switch  automatically
                                                                  land. Also, do not run the engine for more
                            stops the engine when the clip, on the end of
                                                                  than 15 seconds without supplying water,
                            the engine shut-off cord (lanyard), is removed
                                                                  otherwise the engine could overheat.
                            from the switch, such as if the operator falls
                            off the watercraft.                   The start switch (green button) starts the en-
                            Insert the clip  under the engine  shut-off  gine when the switch is pushed.
                            switch before starting the engine.    Release the start switch as soon as the en-
                                                                  gine starts to run. If the engine does not start
                                                        1
                                                                  in 5 seconds, release the start switch, wait 15
                                                                  seconds, and then try again. NOTICE: Never
                                                                  push the start switch while the engine is
                                                             2
                                                                  running. Do not operate the start switch
                                                                  for  more than 5  seconds, otherwise  the
                                                                  battery will be discharged and the engine

                                               3

                              1 Engine shut-off switch
                              2 Clip
                              3 Engine shut-off cord (lanyard)
                            When the engine is not running, remove the
                            clip from the engine shut-off switch to pre-

                                                                                                   32

| 32 33 34 35 36 37 38 39 40 41 42 |