Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 36 - LIT-18626-12-10
P. 36

    UF3V10E0.book  Page 31  Thursday, August 23, 2018  9:17 AM

                            Control function operation

                            EJU31026                              (2) Tap the lock or unlock mode indicator on
                              Watercraft control functions
                                                                     the multifunction information center.
                            EJU45090
                            Yamaha Security System                (3) Flick up or down to set each digit of the
                            The  Yamaha  Security System functions to  4-digit PIN, and then tap the “Enter” but-
                            help prevent unauthorized use or theft of the  ton.
                            watercraft. The lock and unlock modes of the
                            security system can  be selected  using  the
                            engine lock screen of the multifunction infor-    Enter PIN
                            mation center. The engine cannot be started   9    9     9     9
                            if the lock mode of the security system is se-  0  0     0     0
                            lected. The engine can only be started if the  1   1     1     1
                            unlock mode is selected.
                                                                                 Enter
                            TIP:
                            The  Yamaha Security  System setting  can
                            only be selected while the engine is stopped.
                            EJU45100                              TIP:
                            Yamaha Security System setting        The default setting for the PIN is “1234”. The
                            The Yamaha Security System setting can be
                                                                  PIN can also be changed. (See page 50 for in-
                            confirmed by the lock or unlock mode indica-
                                                                  formation on changing the PIN.)
                            tor on the multifunction information center.
                                                                  (4) Tap “ON” to select the lock mode of the
                                                           1         Yamaha Security System or tap “OFF” to
                                                                     select the  unlock mode, and  then  tap
                                                                     “Save”.
                                                           2
                                                                            Engine Lock

                              1 Lock mode indicator
                                                                            ON          OFF
                              2 Unlock mode indicator
                            To  select the lock or unlock mode of the
                                                                                 Save
                            Yamaha Security System:
                            (1) Stop the engine.
                            TIP:
                            If the multifunction  information center is
                                                                  (5) The beeper sounds once when the lock
                            turned off because the engine is stopped,
                                                                     mode of the Yamaha Security System is
                            perform one  of  the following operations to
                                                                     selected and two times when the unlock
                            turn on the center without starting the engine.
                                                                     mode is selected, and the multifunction
                             Push the start switch briefly.
                                                                     information center returns to the home
                             While  pushing the  engine stop switch,
                                                                     screen.
                              push the start switch.

                            31

| 31 32 33 34 35 36 37 38 39 40 41 |