Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 47 - LIT-18626-12-10
P. 47

    UF3V10E0.book  Page 42  Thursday, August 23, 2018  9:17 AM

                                                                      Watercraft operation

                            Activating and deactivating the no-wake   tings: “No Wake –1”, “No Wake” (stan-
                            mode                                     dard setting), and “No Wake +1”.
                            The activation of the no-wake mode can be  To deactivate the no-wake mode:
                            confirmed by the no-wake mode indicator on  Perform one of the following operations. The
                            the multifunction information center.  beeper sounds two times and the no-wake
                                                                  mode indicator  disappears when  the no-
                                                                  wake mode is deactivated.
                                                                   Push the “NO-WAKE MODE” switch.
                                                                   Squeeze the throttle lever.
                                                     MPH           Squeeze the RiDE lever.

                                        No Wake  +1               TIP:
                               0                          100%
                                                                  The no-wake mode is also deactivated when
                                13.6V           x100       F      the engine is stopped.
                                                RPM
                                                                  EJU45031
                                            1     2               Drive control mode
                              1 No-wake mode indicator            The drive control mode is a function for set-
                              2 No-wake mode level
                                                                  ting the maximum watercraft speed and ac-
                            To activate the no-wake mode:         celeration for stable towing and to support
                            (1) Shift into neutral, or release the throttle  inexperienced operators.
                                lever and let the engine speed return to  The maximum watercraft speed can be se-
                                idle.                             lected from three settings and the accelera-
                            (2) Push and hold the “NO-WAKE MODE”  tion can be selected from two settings.
                                switch.  Once the beeper sounds three  TIP:
                                times and the no-wake mode indicator is  The watercraft speed setting is a target value.
                                displayed, the no-wake mode is activat-  The actual watercraft speed may vary de-
                                ed.                               pending on the operating conditions.

                                          1                       Activating the drive control mode
                                                                  Activation of the drive control mode can be
                                                                  confirmed by the drive control mode indica-
                                                       2
                                                                  tor on the multifunction information center.
                                                       3          When the drive control mode is activated, the
                                                                  drive control mode indicator is shown in light
                                                                  blue.

                                                                                   1

                              1 “NO-WAKE MODE” switch
                              2 “SPEED CONTROL” up switch          1 Drive control mode indicator
                              3 “SPEED CONTROL” down switch
                                                                  To activate the drive control mode:
                            (3) Push the “SPEED CONTROL” up switch  (1) Release the throttle lever and let the en-
                                or “SPEED CONTROL” down switch to    gine speed return to idle.
                                adjust the engine speed to  three set-

                                                                                                   42

| 42 43 44 45 46 47 48 49 50 51 52 |