Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 115 - LIT-18626-12-10
P. 115

    UF3V10E0.book  Page 110  Thursday, August 23, 2018  9:17 AM

                                                                           Trouble recovery

                                                                  To tow the watercraft:
                              Fuse amperage:
                                Electronic throttle valve fuse:   Use a towline that is three times the com-
                                  10 A                            bined length of the towing boat and the wa-
                                Fuel pump fuse:                   tercraft.
                                  10 A                            (1) Securely attach the towline to the bow
                                Main relay drive fuse:
                                  10 A                               eye of the watercraft being towed.
                                Main fuse:
                                  20 A
                                Battery fuse:
                                  30 A
                                SCU fuse:
                                  50 A

                            (7) Securely install the fuse box cover in its
                                original position.                    1
                            (8) Securely install the electrical box cover in
                                its original position.
                                                                   1 Bow eye
                            (9) Slide the locks to their original positions
                                to securely lock the electrical box cover  (2) Sit astride the seat and hold on to the
                                in place.                            handlebars in order to balance the water-
                            (10) Securely install the removable watertight  craft. NOTICE: The bow must be kept
                                storage compartment and seats in their  up out of the water during towing, oth-
                                original positions.                  erwise water could  flood the  engine
                            If the fuse immediately blows again, the elec-  compartment or  water could flow
                            trical system may be defective. If this occurs,  back into the engine, causing severe
                            have a Yamaha dealer service the watercraft.  engine damage. [ECJ01331]
                            EJU34716                              Tow the watercraft at 8 km/h (5 mph) or less.
                            Towing the watercraft
                                                                  NOTICE: Tow the watercraft at 8 km/h (5
                            EWJ00812
                                                                  mph) or less, otherwise water could flood
                                 WARNING
                                                                  the engine  compartment or water could
                             The  operator of the  towing boat must
                                                                  flow back into the engine, causing severe
                              keep  speed to a minimum  and avoid
                                                                  engine damage. [ECJ01322]
                              traffic or obstacles which could be  a
                                                                  EJU36156
                              hazard to  the operator  on the water-  Submerged watercraft
                              craft.                              If the watercraft is submerged or flooded with
                             The towline should be long enough so  water, drain the bilge water from the engine
                              that the watercraft will not collide with  compartment. Then, have a Yamaha dealer
                              the towing boat when slowing down.  service the watercraft as soon as possible.
                                                                  If the watercraft was submerged:
                            If the watercraft becomes inoperative in the
                                                                  (1) Remove the watercraft from  the water
                            water, it can be towed to shore.
                                                                     and drain  the water  from the  storage
                                                                     compartments. (See page 58 for  infor-

                                                                                                 110

| 110 111 112 113 114 115 116 117 118 119 120 |