Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 50 - LIT-18626-12-10
P. 50

    UF3V10E0.book  Page 45  Thursday, August 23, 2018  9:17 AM

                            Watercraft operation

                            Activating and deactivating the cruise as-  squeezed further than the position at
                            sist                                     which the cruise assist was set.
                            Activation of the cruise assist can be con-
                                                                  TIP:
                            firmed by the cruise assist indicator on the
                                                                  Check the multifunction information center to
                            multifunction information center.
                                                                  make sure that the cruise assist is activated
                                                                  before squeezing the throttle lever to the full
                                                                  throttle position. If the cruise assist is not ac-
                                                                  tivated, the engine will respond normally to
                                                                  the throttle operation.
                                                     MPH
                                                                  (4) Once the cruise assist is activated, push
                                      Cruise Assist  +4              the “SPEED CONTROL” up switch to in-
                               0                          100%
                                                                     crease the set  engine  speed or  the
                                13.6V           x100       F         “SPEED CONTROL” down switch to de-
                                                RPM
                                                                     crease the set engine speed. The engine
                                            1       2
                                                                     speed can be changed in the range of
                              1 Cruise assist indicator
                                                                     the cruise assist levels –5 to +5.
                              2 Cruise assist level
                            To activate the cruise assist:        TIP:
                            (1) Operate the throttle lever until the de-  Because the cruise assist can only be set be-
                                sired engine speed is reached.    tween engine speeds of approximately 3000
                            (2) When the engine speed reaches the de-  r/min and  approximately 7000 r/min, the
                                sired cruise assist  setting, push the  cruise assist level cannot be adjusted to an
                                “SET” switch. Once the beeper sounds  engine speed outside of this range.
                                three times and the cruise assist indica-  To deactivate the cruise assist:
                                tor is displayed, the cruise assist is acti-  Relax your grip on the throttle lever past the
                                vated.                            position at which the cruise assist was set.
                                                                  The beeper sounds two times and the cruise
                                                                  assist indicator disappears when the cruise
                                                                  assist is deactivated.
                                                       1
                                                       2

                                                       3

                              1 “SPEED CONTROL” up switch
                              2 “SPEED CONTROL” down switch
                              3 “SET” switch
                            (3) When the cruise assist is activated, slow-
                                ly squeeze  the throttle  lever  to keep it

                            45

| 45 46 47 48 49 50 51 52 53 54 55 |