Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 39 - LIT-18626-12-11
P. 39

    UF3X10E0.book  Page 34  Tuesday, August 7, 2018  2:42 PM

                                                             Control function operation

                            zle is changed, and the direction of the water-  EJU31294
                                                                  Adjustable tilt steering system
                            craft is changed accordingly.
                                                                  The position of the handlebars can be adjust-
                                                                  ed back and forth by operating the tilt lever.
                                                1
                                                                  To adjust the handlebar position:
                                                                  (1) Pull the tilt lever up to disengage the han-
                                                                     dlebar lock, and then move the handle-
                                                                     bars back or forth to the desired position.
                                                                     WARNING! Never pull the tilt lever dur-
                                                                     ing operation, otherwise the handle-
                                                                     bars may suddenly  change position,
                                                                     which may lead to an accident. [EWJ00042]

                                                        2
                                                                                            1

                              1 Handlebar
                              2 Jet thrust nozzle
                            Since the strength of the jet thrust determines  1 Tilt lever
                            the speed and degree of a turn, throttle must
                            always  be  applied when attempting a  turn,
                            except at trolling speed.
                            This model is equipped with the Yamaha En-
                            gine Management  System (YEMS) that  in-
                            cludes an off-throttle steering (OTS) system.
                            It will activate at planing speeds should you
                            attempt to steer the watercraft after releasing
                            the throttle lever. The OTS system assists in
                            turning by continuing to supply some thrust
                            while the watercraft is decelerating, but you
                            can turn  more sharply if you apply throttle
                            while turning the handlebars. The OTS sys-
                            tem does not function below planing speeds
                            or when the engine is off. Once the engine
                            slows down, the watercraft will no longer turn
                            in response to handlebar input until you apply
                            throttle again or you reach trolling speed.

                                                                                                   34

| 34 35 36 37 38 39 40 41 42 43 44 |