Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 38 - LIT-18626-12-11
P. 38

    UF3X10E0.book  Page 33  Tuesday, August 7, 2018  2:42 PM

                            Control function operation

                            will not start. Also, the starter motor could  EJU43342
                                                                  RiDE lever
                            be damaged. [ECJ01041]
                                                                  When the RiDE lever is squeezed, the reverse
                                                                  gate lowers and the watercraft starts moving
                                                     1
                                                                  in reverse. If the watercraft is moving forward,
                                                                  the watercraft gradually slows down until it
                                                                  stops, and then the watercraft starts moving
                                                                  in reverse.

                                                                                      1

                              1 Start switch
                            The engine will not start under any of the fol-
                            lowing conditions:
                             Lock mode of the Yamaha Security System
                              has been  selected. (See page 31 for
                              Yamaha Security System setting proce-  1 RiDE lever
                              dures.)
                                                                  When the RiDE lever is released, it automati-
                             Clip is removed  from  the engine  shut-off
                                                                  cally returns to its fully closed (idle) position
                              switch.
                                                                  and the reverse gate moves to the neutral po-
                             Throttle lever is squeezed.
                                                                  sition.
                             Throttle lever is malfunctioning.
                                                                  EJU31262
                             RiDE lever is squeezed.             Steering system
                             RiDE lever is malfunctioning.       By turning the handlebars in the direction you
                            EJU31212                              wish to travel, the angle of the jet thrust noz-
                            Throttle lever
                            The throttle lever increases the engine speed
                            when the lever is squeezed.

                                     1

                              1 Throttle lever
                            The throttle lever returns automatically to its
                            fully closed (idle) position when released.

                            33

| 33 34 35 36 37 38 39 40 41 42 43 |