Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 70 - LIT-18626-12-11
P. 70

    UF3X10E0.book  Page 65  Tuesday, August 7, 2018  2:42 PM

                            Operation and handling requirements

                            EJU40291                              (2) Remove the seats. (See page 55 for seat
                                 Engine oil requirements
                                                                     removal and installation procedures.)
                            EJU31897
                            Engine oil                            (3) Remove the dipstick and wipe it clean.
                            ECJ00282
                             NOTICE
                            Use only 4-stroke engine oil. Usage of 2-                        1
                            stroke engine oil could result in severe en-
                            gine damage.

                              Recommended engine oil:
                                YAMALUBE 4W
                              Recommended engine oil type:
                                SAE 10W-30, 10W-40, 20W-40,
                                20W-50
                                                                   1 Dipstick
                              Recommended engine oil grade:
                                API SJ, SL                        (4) Insert the dipstick back into the dipstick
                                                                     tube  completely. Remove the  dipstick
                            TIP:                                     again and make sure that the engine oil
                            When the engine is operated at high speeds,  level is between the minimum and maxi-
                            some engine oil may be consumed. Be sure  mum level marks.
                            to check the engine oil level.
                            Checking the engine oil level
                            EWJ00341
                                 WARNING
                            Engine oil is extremely hot immediately af-
                                                                                          1
                            ter the engine is turned off. Coming in con-
                            tact with or getting any engine oil on your                   2
                            clothes could result in burns.

                            ECJ01002
                             NOTICE
                                                                   1 Maximum level mark
                            Make sure  that debris and  water  do not  2 Minimum level mark
                            enter the oil filler hole. Debris and water in
                                                                  (5) If the engine oil  level  is  significantly
                            the engine oil  can cause serious engine
                                                                     above the maximum level mark, consult
                            damage.
                                                                     a Yamaha dealer. If the engine oil level is
                            To check the engine oil level:           below the minimum level mark, add en-
                            (1) Place the watercraft in a precisely level  gine oil.
                                position on land with the  engine
                                stopped. If the engine was running, allow
                                the engine oil to settle by waiting 5 min-
                                utes or more before checking the oil lev-
                                el.

                            65

| 65 66 67 68 69 70 71 72 73 74 75 |