Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 67 - LIT-18626-12-11
P. 67

    UF3X10E0.book  Page 62  Tuesday, August 7, 2018  2:42 PM

                                                                     Equipment operation

                            EJU42391                                 hood is securely closed before using the
                            Fire extinguisher holder and cover
                                                                     watercraft.
                            The fire extinguisher holder and cover are lo-
                            cated in the bow storage compartment.
                            To use the fire extinguisher holder and cover:
                            (1) Pull the hood latch rearward, and then lift
                                up the rear of the hood.
                                                      1

                                                                  EJU45291
                                                                  Optional part mounting bracket
                                                                  A mounting bracket  for installing  optional
                                                                  parts is located near the port (left) side of the
                                                                  multifunction information center.
                              1 Hood latch
                            (2) Unhook the band and remove the fire ex-
                                                                           1
                                tinguisher cover.

                                                   1

                                                   2
                                                                   1 Optional part mounting bracket
                                                                    Load limit:
                                                                      1.0 kg (2.2 lb)
                              1 Fire extinguisher holder and cover
                              2 Band
                            (3) Place the fire extinguisher in the holder,
                                and then place the cover over the fire ex-
                                tinguisher.
                            (4) Securely fasten the cover and the fire ex-
                                tinguisher with the band.
                            (5) Push the rear of the hood down to se-
                                curely lock it in place. Make sure that the

                                                                                                   62

| 62 63 64 65 66 67 68 69 70 71 72 |