Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 114 - LIT-18626-12-11
P. 114

    UF3X10E0.book  Page 109  Tuesday, August 7, 2018  2:42 PM

                            Trouble recovery

                            (3) Remove the electrical box cover.     Install the spare fuse,  and then  tighten
                                                                     the screws.
                                  1                         3
                                                                     1 23       4  5       6 7

                                                          2                                     8
                                                        2                                       9
                                                   3

                                                                                                8
                              1 Electrical box cover                           10     5
                              2 Lock                               1 Electronic throttle valve fuse
                              3 Projection                         2 Fuel pump fuse
                            (4) While pushing both sides of the fuse box  3 Main relay drive fuse
                                                                   4 Main fuse
                                cover inward, pull the cover toward the
                                                                   5 Spare fuse
                                bow and remove it.
                                                                   6 Fuse puller
                                                                   7 Battery fuse
                                    1                              8 Screw
                                                                   9 SCU fuse (BCU fuse)
                                                                  10 Unused fuse
                                                                  (6) When  replacing a fuse other than the
                                                                     SCU fuse, remove the  fuse  using the
                                                                     fuse puller. Install a spare fuse of the
                                                                     proper amperage.  WARNING! Do not
                                                                     use fuses of a different amperage than
                                                                     recommended. Substitution with  a
                              1 Fuse box cover
                                                                     fuse that has an improper rating can
                            (5) When replacing the SCU fuse, remove
                                                                     cause extensive electrical  system
                                the screws, and then remove the fuse.
                                                                     damage and possible fire. [EWJ00803]

                            109

| 109 110 111 112 113 114 115 116 117 118 119 |