Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 103 - LIT-18626-12-11
P. 103

    UF3X10E0.book  Page 98  Tuesday, August 7, 2018  2:42 PM

                                                                                 Maintenance

                            (3) Lift up the engine cover to remove it.

                                            1

                              1 Engine cover
                            To install the engine cover:
                            (1) Place the engine cover in its original po-
                                sition, and then push it down.

                            (2) Install the engine cover screws.
                            (3) Securely install the seats in their original
                                positions.

                                                                                                   98

| 98 99 100 101 102 103 104 105 106 107 108 |