Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 22 - LIT-18626-12-11
P. 22

    UF3X10E0.book  Page 17  Tuesday, August 7, 2018  2:42 PM

                                Safety information

                              ther  direction, although some  movement   Stop the engine and remove the clip from
                              may occur.                           the engine shut-off switch before removing
                                                                   any debris or weeds, which may have col-
                                                                   lected around the jet intake.
                                                                                               2
                                                     MPH

                               0                          100%
                                                                             1
                                13.6V           x100       N
                                                RPM
                                                           1
                              1 “N” (Neutral position)
                             To avoid rear-end collisions while operat-
                              ing the watercraft, check behind you be-  1 Clip
                                                                   2 Engine shut-off switch
                              fore using the RiDE lever to slow down or
                              stop the watercraft. Make sure that there
                              are no obstacles or people behind you be-
                              fore shifting into reverse.
                             Keep away from the intake grate while the
                              engine is on. Items such as long hair, loose
                              clothing, or PFD straps can become entan-
                              gled in moving parts, resulting in severe in-
                              jury or drowning.
                             Never insert any object into the jet thrust
                              nozzle while the engine is running. Severe
                              injury or death could result from coming in
                              contact with the rotating parts  of the jet
                              pump.

                                                           2

                                                   1

                              1 Intake grate
                              2 Jet thrust nozzle

                            17

| 17 18 19 20 21 22 23 24 25 26 27 |