Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 61 - LIT-18626-12-12
P. 61

    UF3P12E0.book  Page 56  Monday, July 23, 2018  9:51 AM

                                             Operation and handling requirements

                            (4) Pull the hood latch up, and then lift up  of the fuel tank. Do not overfill the fuel
                                the rear of the hood.                tank. Because fuel expands when it
                                                                     heats up, heat from the engine or the sun
                             1                                       can cause fuel to spill out of the fuel tank.
                                                                     Do not  leave the watercraft with  a full
                                                                     tank in direct sunlight.
                                                                             1

                              1 Hood latch
                            (5) Loosen the fuel filler cap and remove it.

                                                                   1 Top of the fuel tank

                                                                                            1
                                                                                                 2

                                              1
                              1 Fuel filler cap
                            (6) Slowly add fuel to the fuel tank.
                              Fuel tank capacity:                  1 Top of the fuel tank
                                70 L (18.5 US gal, 15.4 Imp.gal)   2 Approximately 50 mm (2 in) from top of the
                                                                     fuel tank
                                                                  (8) Wipe up any spilled fuel immediately with
                                                                     a dry cloth.
                                                                  (9) Securely install the fuel filler cap by tight-
                                                                     ening it until it clicks.
                                                                  (10) Return the hood to its original position,
                                                                     and then push the hood latch down to
                                                                     securely lock it in place. Make sure that
                                                                     the fuel filler cap and the hood are se-

                            (7) Stop filling  when the  fuel level reaches
                                approximately 50 mm (2 in) from the top

                                                                                                   56

| 56 57 58 59 60 61 62 63 64 65 66 |