Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 94 - LIT-18626-12-12
P. 94

    UF3P12E0.book  Page 89  Monday, July 23, 2018  9:51 AM

                            Maintenance

                            EJU33758                              nance not covered by this owner’s/operator’s
                                       Maintenance
                                                                  manual.
                            Periodic  checks and  lubrication will keep  EJU33803
                            your watercraft in the safest and most effi-  Tool kit
                            cient condition  possible. Therefore, make  A tool kit is included with  this watercraft.
                            sure to carry out the periodic maintenance.  Place the tool kit in a waterproof bag and al-
                            Safety is an obligation of the watercraft own-  ways carry it with you whenever you use the
                            er. Proper maintenance must be carried out  watercraft.
                            to keep the exhaust emission and sound lev-
                            els within the regulated limits. The most im-
                            portant points of watercraft inspection  and
                            lubrication are explained on the following
                            pages.
                            See a Yamaha dealer for genuine Yamaha re-
                            placement parts and  optional accessories
                            designed for your watercraft.
                            Remember, failures that are the result of the
                            installation of parts or accessories which are
                                                                   1 Tool bag
                            not qualitatively equivalent  to genuine
                                                                   2 Screwdriver
                            Yamaha parts are not covered by the limited
                                                                   3 Garden hose adapter
                            warranty.
                                                                   4 10/12 mm box wrench
                            Maintenance, replacement, or repair of  5 Pliers
                            the emission control devices and system  6 10/12 mm open-end wrench
                            may be performed by any marine SI engine
                                                                  EJU42023
                            repair  establishment or individual.  War-  Removing and installing the engine
                            ranty repair, however, must be performed  cover
                            at an authorized Yamaha  marine dealer-  The engine cover is removable.
                            ship.                                 To remove the engine cover:
                            EWJ00312                              (1) Remove the seats. (See page 48 for seat
                                 WARNING                             removal and installation procedures.)
                            Be sure to turn off the engine when you  (2) Remove the engine cover screws.
                            perform maintenance  unless otherwise                1
                            specified. If you are not familiar with ma-
                            chine servicing, this work should be done
                            by a Yamaha dealer or other qualified me-
                            chanic.

                            A service  manual is  available for  purchase
                            through a  Yamaha dealer  for owners  who
                            have the mechanical skills, tools, and other
                            equipment necessary to perform  mainte-
                                                                   1 Engine cover screw

                            89

| 89 90 91 92 93 94 95 96 97 98 99 |