Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 95 - LIT-18626-12-12
P. 95

    UF3P12E0.book  Page 90  Monday, July 23, 2018  9:51 AM

                                                                                 Maintenance

                            (3) Lift up the engine cover to remove it.

                                            1

                              1 Engine cover
                            To install the engine cover:
                            (1) Place the engine cover in its original po-
                                sition, and then push it down.

                            (2) Install the engine cover screws.
                            (3) Securely install the seats in their original
                                positions.

                                                                                                   90

| 90 91 92 93 94 95 96 97 98 99 100 |