Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 59 - LIT-18626-12-12
P. 59

    UF3P12E0.book  Page 54  Monday, July 23, 2018  9:51 AM

                                                                     Equipment operation

                            To use the fire extinguisher holder and cover:  the hood is securely closed before using
                            (1) Pull the hood latch up, and then lift up  the watercraft.
                                the rear of the hood.

                             1

                              1 Hood latch
                            (2) Unhook the band and remove the fire ex-
                                tinguisher from the fire extinguisher cov-
                                er.

                                                           1

                                                           2

                              1 Band
                              2 Fire extinguisher holder and cover
                            (3) Place the fire extinguisher in the fire ex-
                                tinguisher cover, and then securely fas-
                                ten the fire extinguisher with the band.
                            (4) Return the hood to its original position,
                                and then push the hood latch down to
                                securely lock it in place. Make sure that

                                                                                                   54

| 54 55 56 57 58 59 60 61 62 63 64 |