Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 90 - LIT-18626-12-13
P. 90

    UF2W15E0.book  Page 85  Monday, July 9, 2018  4:26 PM

                            Care and storage

                                ter flows out continually from  the  jet  NOTICE: Do not use high-pressure
                                thrust nozzle.                       water when rinsing the engine or en-
                                                                     gine  compartment as severe engine
                                                                     damage could result. [ECJ00572]
                                                                  (3) Drain  the water  from the engine com-
                                                                     partment. (See page 59 for information
                                                                     on draining the bilge water.)
                                                                  (4) Wipe  the engine  and engine compart-
                                                                     ment with a dry cloth.
                                                                  (5) Wash down the hull, deck, and jet pump
                                                                     with fresh water.
                                                                  (6) Wipe the hull, deck, and jet pump with a
                            (7) Run the engine at idling speed for about  dry cloth.
                                3 minutes watching the engine condition.  (7) Wipe  all vinyl and rubber components,
                                If the  engine stops  while flushing,  turn  such as the seats and engine compart-
                                the water supply off immediately  and  ment seals, with a vinyl protectant such
                                perform the procedure again from step 6.  as Yamaclean Vinyl Dressing™.
                                NOTICE: Do not supply water to the  (8) To minimize corrosion, spray metallic
                                cooling water passages when the en-  parts of the hull, deck, and engine with a
                                gine is not running. The water could  rust inhibitor such as Yamalube Silicone
                                flow back through the muffler into the  Protectant & Lubricant.
                                engine, causing severe engine  dam-  (9) Allow the engine compartment to air dry
                                                                     completely before installing the seats.
                                age. [ECJ00123]
                            (8) Turn the water supply off.        (10) Securely install the seats in their original
                            (9) Discharge the remaining water out of the  positions.
                                cooling  water passages by  alternately  EJU41632
                                                                  Battery care
                                squeezing and releasing the throttle lever
                                                                  If the watercraft will not be used for more than
                                quickly for 10 to 15 seconds.
                                                                  a month, remove the battery from the water-
                            (10) Stop the engine.
                                                                  craft, check it, and then store it in a cool, dry
                            (11) Remove the garden hose adapter, and
                                                                  place.
                                then securely install the flushing hose  EWJ00792
                                connector cap  by tightening  it until it  WARNING
                                stops.
                                                                  Battery electrolyte is poisonous and dan-
                            (12) Securely install the removable watertight
                                                                  gerous, causing severe burns, etc. Elec-
                                storage compartment and seats in their
                                                                  trolyte contains sulfuric acid. Avoid
                                original positions.
                                                                  contact with skin, eyes, or clothing.
                            EJU33747
                            Cleaning the watercraft               Antidotes
                            (1) Remove the seats. (See page 48 for seat  External: Flush with water.
                                removal and installation procedures.)  Internal: Drink large quantities of water or
                            (2) Rinse the engine and engine compart-  milk. Follow with milk of magnesia, beaten
                                ment with a small amount  of  water.
                            85

| 85 86 87 88 89 90 91 92 93 94 95 |