Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 97 - LIT-18626-12-13
P. 97

    UF2W15E0.book  Page 92  Monday, July 9, 2018  4:26 PM

                                                                                 Maintenance

                                                                   Initial    Thereafter every
                                                                                   100    200
                                                                         50 hours
                                   Item             Operation              or 12   hours or  hours or   Page
                                                                  10 hours         12      24
                                                                          months
                                                                            *1   months  months
                                                                                   *1      *1
                                              Check for exhaust leak-
                             Exhaust system   age, and check hoses and              √            —
                                              clamps
                                              Check breather hose and
                             Breather hose                                          √            —
                                              clamps
                                              Check for bends, dam-
                             Impeller                                               √            —
                                              age, and foreign material
                                              Check movement, and lu-
                             Jet thrust nozzle                                      √            —
                                              bricate
                                              Check hoses for clogs
                                              and damage, check
                             Jet vacuum bilge                                       √            —
                                              clamps, and clean bilge
                                              strainer
                             Stern drain plugs  Check O-rings                       √            —
                                              Check for corrosion, and
                             Anode                                                        √ *2   —
                                              clean
                             Valve clearance  Check and adjust                            √ *2   —
                                              Check for cracks, inden-
                             Rubber coupling  tations, looseness, and                      √     —
                                              noise
                                              Check for damage and
                             Engine mount                                                  √     —
                                              peeling
                            *1: Whichever comes first.
                            *2: Check every 200 hours.
                            Perform the pre-operation checks and  post-operation checks  before  performing  periodic
                            maintenance.

                                                                                                   92

| 92 93 94 95 96 97 98 99 100 101 102 |