Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 48 - LIT-18626-12-13
P. 48

    UF2W15E0.book  Page 43  Monday, July 9, 2018  4:26 PM

                            Instrument operation

                            EJU43760                              their state before the center turned off, and
                                Multifunction information
                                                                  then the center starts to operate normally.
                                          center                  EJU35027
                                                                  Information display
                            The multifunction information center displays
                                                                  The information display shows watercraft op-
                            various watercraft information.
                                                                  erating conditions.
                                      1      2      3
                                                                          1    2     3

                                             4
                              1 “UNLOCK” indicator light                    4 5 6 7  8  9
                                                                   1 Trim indicator
                              2 Information display
                                                                   2 Tachometer
                              3 “L-MODE” indicator light
                                                                   3 Speedometer
                              4 “WARNING” indicator light
                                                                   4 Oil pressure warning indicator
                            Multifunction information center initial op-
                                                                   5 Engine overheat warning indicator
                            eration
                                                                   6 Check engine warning indicator
                            When the multifunction information center is
                                                                   7 Shift indicator
                            activated, all of the display segments come  8 Fuel level warning indicator
                            on. After 2 seconds, the warning indicators in  9 Fuel level meter
                            the information display go off, and then the
                                                                  EJU43832
                            center starts to operate normally.    Speedometer
                            If only the multifunction information center is  The speedometer shows the watercraft
                            activated, the “WARNING” indicator light  speed against water.
                            blinks once.
                            TIP:
                            The “UNLOCK” indicator light also comes on
                            as part of the initial operation.
                            The  “UNLOCK” indicator light will go off
                            when the engine is started.
                            Multifunction information center standby
                            state
                            If the  multifunction information center  does
                                                                                     1
                            not receive any operation input within 25 sec-
                                                                   1 Speedometer
                            onds after the engine stops, the center will
                            turn off and enter a standby state. When the  By switching the display units, the speed can
                            engine is started again, the displays return to  be shown in kilometers per hour “km/h” or
                                                                  miles per hour “MPH”.

                            43

| 43 44 45 46 47 48 49 50 51 52 53 |