Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 72 - LIT-18626-12-13
P. 72

    UF2W15E0.book  Page 67  Monday, July 9, 2018  4:26 PM

                            Pre-operation checks

                            right and left fully turned positions of the jet  lever returns automatically to its fully closed
                            thrust nozzle.                        position when released.

                                                                  EJU42181
                                                                  Throttle lever checks
                                                                  Operate the throttle lever several times to
                                                                  make sure that operation is smooth through-
                                                                  out the whole range. Also, make sure that the
                                                                  throttle lever returns automatically to its fully
                                                                  closed (idle) position when released.

                                                                  EJU40113
                                                                  Remote control transmitter check
                              Difference between fully turned posi-  Make sure that the remote control transmitter
                              tions of jet thrust nozzle (distances A
                              and B):                             operates properly. (See page 32 for Yamaha
                                Maximum 5 mm (0.20 in)            Security System setting procedures and
                                                                  page 41 for Low RPM Mode activation pro-
                            EJU43213                              cedures.)
                            RiDE lever checks
                                                                  EJU32664
                            Operate the RiDE lever several times to make  Engine shut-off cord (lanyard) check
                            sure that operation is smooth throughout the  Make sure that the engine shut-off cord (lan-
                            whole range. Also, make sure that the RiDE  yard) is not damaged. If the cord is damaged,
                                                                  replace it.  WARNING! Never try to repair
                                                                  the engine shut-off cord (lanyard) or tie it
                                                                  together. The  engine  shut-off cord (lan-

                            67

| 67 68 69 70 71 72 73 74 75 76 77 |