Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 106 - LIT-18626-12-14
P. 106

    UF4E13E0.book  Page 101  Friday, April 27, 2018  2:35 PM

                            Trouble recovery

                            (1) Connect the positive (+) jumper cable to  EJU44050
                                                                  Replacing the fuses
                                the positive (+) battery terminals of both
                                                                  If a fuse is blown, replace it with the proper
                                batteries.
                                                                  fuse.
                            (2) Connect one  end of the negative  (–)
                                jumper cable to the negative (–) battery  1          2
                                terminal of the booster battery.
                            (3) Connect the other end of the negative (–)
                                jumper cable to an engine hanger.
                                                      2    1
                                   3

                                              4
                                                                   1 Good fuse
                                                                   2 Blown fuse

                                                                    1                2
                              1 Positive (+) jumper cable
                              2 Booster battery
                              3 Negative (–) jumper cable
                              4 Engine hanger
                            (4) Start the engine, and then disconnect the
                                jumper cables by reversing  the  steps
                                above. (See page 33 for information on
                                starting the engine.)
                                                                   1 Good fuse
                                                                   2 Blown fuse
                                                                  To replace a fuse:
                                                                  (1) Remove the seats and removable water-
                                                                     tight storage compartment. (See page 49
                                                                     for seat removal and installation proce-
                                                                     dures and page 54 for information on the
                                                                     removable  watertight storage compart-
                                                                     ment.)

                            101

| 101 102 103 104 105 106 107 108 109 110 111 |