Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 44 - LIT-18626-12-14
P. 44

    UF4E13E0.book  Page 39  Friday, April 27, 2018  2:35 PM

                            Watercraft operation

                                                                  EJU40001
                            TIP:                                   Watercraft operation modes
                            If the RiDE lever is squeezed while the throttle
                            lever is squeezed, the  watercraft  will  slow  EJU36787
                            down, and once stopped, move in reverse.  Low RPM Mode
                            To shift into neutral from forward:   The Low RPM Mode is a function that limits
                            (1) Release the throttle lever.       the maximum engine speed to approximately
                            (2) Lightly squeeze and release the RiDE le-  70% of the maximum engine speed in the
                                ver. The “N” (neutral) shift indicator will  normal mode.
                                be displayed.                     The Low RPM Mode can only be activated
                                                                  and  deactivated by operating the  remote
                                                                  control transmitter that is included with this
                                                                  watercraft. (See page 31 for information on
                                                                  the remote control transmitter.)

                                                                   1 Remote control transmitter
                                                                  TIP:
                                                                  The Low RPM Mode can only be activated
                                                                  when  the  engine is stopped in the unlock
                                                                  mode of the Yamaha Security System.
                                             1                    Activating and deactivating the Low RPM
                              1 “N” (Neutral position)            Mode
                                                                  Activation of the Low RPM Mode will be con-
                            TIP:
                                                                  firmed by the number of beeps when the re-
                            If the RiDE lever is squeezed continuously,
                                                                  mote control transmitter is operated, and by
                            the reverse gate will move to the reverse po-
                                                                  the “L-MODE” indicator light of the multifunc-
                            sition.
                                                                  tion information center. (See page 44 for in-
                                                                  formation  on the multifunction  information
                                                                  center.)

                            39

| 39 40 41 42 43 44 45 46 47 48 49 |