Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 92 - LIT-18626-12-14
P. 92

    UF4E13E0.book  Page 87  Friday, April 27, 2018  2:35 PM

                            Care and storage

                            egg, or vegetable oil. Call a physician im-  Checking the electrolyte level
                            mediately.                            Make sure  that the electrolyte level is be-
                            Eyes: Flush with water for 15 minutes and  tween the maximum  and  minimum level
                            get prompt medical attention.         marks.
                            Batteries produce explosive gases. Keep  If the electrolyte level is low, add distilled wa-
                            sparks, flames, cigarettes, etc., well away.  ter to raise it to the specified level. NOTICE:
                            If using or charging the battery in an en-  Use only distilled water for  replenishing
                            closed space, make sure that it is well  the battery, otherwise battery life could be
                            ventilated. Always shield your eyes when  shortened. [ECJ00242]
                            working near batteries.
                            Keep out of the reach of children.

                            To remove the battery:
                            (1) Disconnect the negative (–) battery lead.
                            (2) Disconnect the positive (+) battery lead.
                            (3) Disconnect the breather hose.
                            (4) Unhook the battery bands, and then re-
                                move the battery from the watercraft.

                             1  2       3                          1 Maximum level mark
                                                                   2 Minimum level mark
                                                                  If distilled water was added, check the bat-
                                                                  tery voltage.
                                        4                         It is recommended to have a Yamaha dealer
                                                                  check the battery voltage and charge the bat-
                                                                  tery. If you  charge the battery  yourself, be
                                                                  sure to read and follow the instructions pro-
                                                                  vided with the battery tester and charger you
                              1 Negative (–) battery terminal: Black lead
                                                                  use. NOTICE: Do not attempt to charge a
                              2 Battery band
                                                                  battery hastily. Battery life could be short-
                              3 Positive (+) battery terminal: Red lead
                              4 Breather hose                     ened. [ECJ00252]
                            Checking the battery
                             Make sure that the battery case is not dam-
                              aged.
                             Make  sure that the  battery terminals are
                              not corroded or damaged.
                             Make sure that the breather  hose  is not
                              clogged or damaged.

                            87

| 87 88 89 90 91 92 93 94 95 96 97 |