Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 63 - LIT-18626-12-14
P. 63

    UF4E13E0.book  Page 58  Friday, April 27, 2018  2:35 PM

                                             Operation and handling requirements

                                curely closed before using  the  water-  EJU40291 Engine oil requirements
                                craft.
                                                                  EJU31897
                                                                  Engine oil
                                                                  ECJ00282
                                                                  NOTICE
                                                                  Use only 4-stroke engine oil. Usage of 2-
                                                                  stroke engine oil could result in severe en-
                                                                  gine damage.

                                                                    Recommended engine oil:
                                                                      YAMALUBE 4W
                                                                    Recommended engine oil type:
                                                                      SAE 10W-30, 10W-40, 20W-40,
                            (11) Securely install the seats in their original  20W-50
                                positions.                          Recommended engine oil grade:
                                                                      API SG, SH, SJ, SL

                                                                  TIP:
                                                                  When the engine is operated at high speeds,
                                                                  some engine oil may be consumed. Be sure
                                                                  to check the engine oil level.
                                                                  Checking the engine oil level
                                                                  EWJ00341
                                                                      WARNING
                                                                  Engine oil is extremely hot immediately af-
                                                                  ter the engine is turned off. Coming in con-
                                                                  tact with or getting any engine oil on your
                                                                  clothes could result in burns.

                                                                  ECJ01002
                                                                  NOTICE
                                                                  Make sure  that debris and  water  do not
                                                                  enter the oil filler hole. Debris and water in
                                                                  the engine oil can cause serious engine
                                                                  damage.
                                                                  To check the engine oil level:
                                                                  (1) Place the watercraft in a precisely level
                                                                     position  on land with the engine
                                                                     stopped. If the engine was running, allow
                                                                     the engine oil to settle by waiting 5 min-
                                                                     utes or more before checking the oil lev-
                                                                     el.

                                                                                                   58

| 58 59 60 61 62 63 64 65 66 67 68 |