Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 36 - LIT-18626-12-14
P. 36

    UF4E13E0.book  Page 31  Friday, April 27, 2018  2:35 PM

                            Control function operation

                            EJU31026                              in the transmitter holder in the glove compart-
                              Watercraft control functions
                                                                  ment, so that it is not lost.
                            EJU43910
                            Remote control transmitter                                            1
                            The Yamaha Security System and Low RPM
                            Mode settings can be selected by operating
                            the remote control transmitter. (See page 32
                            for Yamaha Security System setting proce-
                            dures and page 39 for Low RPM Mode acti-
                            vation procedures.)

                                                                   1 Transmitter holder
                                                                  ECJ00753
                                                                  NOTICE
                                                                   The remote control transmitter  is  not
                                                                   completely waterproof. Do  not  sub-
                                                                   merge the transmitter or operate it un-
                                                                   derwater.  If  the  transmitter  is
                              1 Remote control transmitter         submerged, dry it with a soft, dry cloth,
                            Since the watercraft is programmed to rec-  and then check that it is operating prop-
                            ognize the internal code from this transmitter  erly. If the transmitter is not operating
                            only, the settings can only be selected with  properly, contact a Yamaha dealer.
                            this transmitter.                      Keep the remote control  transmitter
                            If you accidentally lose your remote control  away from high  temperatures and  do
                            transmitter or if it is not operating properly,  not place it in direct sunlight.
                            contact a Yamaha dealer.               Do not drop the remote control trans-
                            When operating the watercraft, always keep  mitter, subject it to  strong shocks, or
                            the transmitter with you, such as by storing it  place any heavy items on it.
                                                                   Use a soft, dry cloth to clean the remote
                                                                   control  transmitter. Do  not use deter-
                                                                   gent, alcohol, or other chemicals.
                                                                   Do not attempt to disassemble the re-
                                                                   mote control transmitter yourself. Oth-
                                                                   erwise, the transmitter may not operate
                                                                   properly. If the transmitter needs a new
                                                                   battery, contact a Yamaha dealer. Refer
                                                                   to local hazardous  waste regulations
                                                                   when disposing of transmitter batteries.

                                                                  This device complies with Part 15 of the FCC
                                                                  Rules. Operation is subject to the following

                            31

| 31 32 33 34 35 36 37 38 39 40 41 |